# Only for opensmart 2.4inch 240x320 ili9341 lcd screen


The LED pin in opensmart led needs to be 0V to light.

!!!! Only 2.4 inch screen is tx,rx based !!!!

!!!! Only 3.5 inch screen uses a Self_Designed wired protocol, not spi, not uart !!!!
