# Common Emitter

In electronics, a common-emitter amplifier is one of three basic single-stage bipolar-junction-transistor (BJT) amplifier topologies, typically used as the voltage amplifier.

In this circuit the base terminal of the transistor serves as the input, the collector is the output, and the emitter is common to both (for example, it may be tied to ground reference or a power supply rail), hence its name.

A change in base current
produces a corresponding change in collector current,
, and the common emitter gain
is then defined by

之所以讲`共射电路`，是因为后面大多数时候我们能遇到的电路都是这个，而且后面知识的大体框架是一样的，只是细节不一样

# results matching ""

# No results matching ""