# Bipolar Junction Transistor

Bipolar Junction Transistor \(三极管\)

> A `bipolar junction transistor` \(`bipolar transistor` or `BJT`\) is a type of transistor that uses both electron and hole charge carriers.
>
> BJTs use two junctions between two semiconductor types, n-type and p-type.

## 0. 为什么学这个？

因为放大器电路需要它。

Transistor \(晶体管\)

> A semiconductor device with three connections, capable of amplification in addition to rectification.

## 1. 认识你自己（不对，应该是认识一下三极管）

![](../../.gitbook/assets/SanJiGuan1.png)

![](../../.gitbook/assets/SanJiGuan2.png)

![](../../.gitbook/assets/Bipolar_junction_transistor.png)

`E` means `emitter`

`B` means `base`

`C` means `collector`

## 2. 了解更多

![](../../.gitbook/assets/SanJiGuan1.png)

箭头所指方向为电流流动的方向。

学到 PN结 的都知道，电流从正电压出发，由 P 流到 N

## 3. 总结规律

![](../../.gitbook/assets/SanJiGuan1.png)

$$
\begin{align*}
&I_E = I_C + I_B
\\ \\
&I_C  \approx I_E = A \cdot I_B (A > 0)
\\ \\
&\text{# A 是一个系数，反正整个式子表示 } I_C \text{ 是 } I_B \text{ 的 A 倍}
\end{align*}
$$

所以才把`E端`叫做`发射区`啊， 因为三级管在起放大作用时，`E端`输出的电流是最大的。

 **靠近中间那块板子的箭头 所在的部分是 E\(发射区\)，它的对面是 C\(集电区\)，中间永远为 B\(基区\)**

## 4. 升仙（不对，升华）

在讲这个之前，我要先讲讲什么叫做`正偏`、什么叫做`反偏`（当然，都是一个名字、代号而已）

正偏：$$U_p > U_n$$

反偏：$$U_p < U_n$$

比如：

正偏就是指`PN结`中的`P端`电压大于`N端`，也就是正向导通

反偏就是指`PN结`中的`P端`电压小于`N端`，也就是反向导通了。

于是乎，在三级管起放大作用时\(他们称它正处在`整个元件输出函数图`的`放大区`\)

此时：`EB结(发射结)`正偏；`CB结(集电结)`反偏

饱和区：`EB结(发射结)`正偏；`CB结(集电结)`正偏

截止区：`EB结(发射结)`反偏；`CB结(集电结)`反偏

## 5. 记忆秘诀

带箭头的是B\(射极\)

B的对面是C\(集极\)

中间那个自然就是B\(基极\)

